Chris Golpashin

April 6, 2016

UNIX/Linux Administration

Lab 10

Installing Various Linux Distros

Our server had a total of 24 GBs of RAM. It had two Quad core Xeon CPUs which is a total of 8 cores. It uses a RAID card with a separate BIOS. I don’t remember the MAC addresses of the two Ethernet ports. We were able to install debian 8 directly using keyboard, mouse, and monitor. The storage drives needed to be setup in the RAID BIOS even if it was a single drive. The OS install automatically configured the network setup with the MAC address of the Ethernet port.